TurboJPEG 1.5

- Main Page
- Modules
- Data Structures

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups
Data Structures | Macros | Typedefs | Enumerations | Functions | Variables
TurboJPEG

TurboJPEG API. More...

## Data Structures

struct | tjscalingfactor
| Scaling factor. More...
struct | tjregion
| Cropping region. More...
struct | tjtransform
| Lossless transform. More...

## Macros

#define | TJ_NUMSAMP
| The number of chrominance subsampling options. More...
#define | TJ_NUMPF
| The number of pixel formats. More...
#define | TJ_NUMCS
| The number of JPEG colorspaces. More...
#define | TJFLAG_BOTTOMUP
| The uncompressed source/destination image is stored in bottom-up (Windows, OpenGL) order, not top-down (X11) order. More...
#define | TJFLAG_FASTUPSAMPLE
| When decompressing an image that was compressed using chrominance subsampling, use the fastest chrominance upsampling algorithm available in the underlying codec. More...
#define | TJFLAG_NOREALLOC
| Disable buffer (re)allocation. More...
#define | TJFLAG_FASTDCT
| Use the fastest DCT/IDCT algorithm available in the underlying codec. More...
#define | TJFLAG_ACCURATEDCT
| Use the most accurate DCT/IDCT algorithm available in the underlying codec. More...
#define | TJ_NUMXOP
| The number of transform operations. More...
#define | TJXOPT_PERFECT
| This option will cause tjTransform() to return an error if the transform is not perfect. More...
#define | TJXOPT_TRIM
| This option will cause tjTransform() to discard any partial MCU blocks that cannot be transformed. More...
#define | TJXOPT_CROP
| This option will enable lossless cropping. More...
#define | TJXOPT_GRAY
| This option will discard the color data in the input image and produce a grayscale output image. More...
#define | TJXOPT_NOOUTPUT
| This option will prevent tjTransform() from outputting a JPEG image for this particular transform (this can be used in conjunction with a custom filter to capture the transformed DCT coefficients without transcoding them.) More...
#define | TJPAD(width)
| Pad the given width to the nearest 32-bit boundary. More...
#define | TJSCALED(dimension, scalingFactor)
| Compute the scaled value of `dimension` using the given scaling factor. More...

## Typedefs

typedef struct tjtransform | tjtransform
| Lossless transform. More...
typedef void * | tjhandle
| TurboJPEG instance handle. More...

## Enumerations

enum | TJSAMP { TJSAMP_444, TJSAMP_422, TJSAMP_420, TJSAMP_GRAY, TJSAMP_440, TJSAMP_411 }
| Chrominance subsampling options. More...
enum | TJPF { TJPF_RGB, TJPF_BGR, TJPF_RGBX, TJPF_BGRX, TJPF_XBGR, TJPF_XRGB, TJPF_GRAY, TJPF_RGBA, TJPF_BGRA, TJPF_ABGR, TJPF_ARGB, TJPF_CMYK }
| Pixel formats. More...
enum | TJCS { TJCS_RGB, TJCS_YCbCr, TJCS_GRAY, TJCS_CMYK, TJCS_YCCK }
| JPEG colorspaces. More...
enum | TJXOP { TJXOP_NONE, TJXOP_HFLIP, TJXOP_VFLIP, TJXOP_TRANSPOSE, TJXOP_TRANSVERSE, TJXOP_ROT90, TJXOP_ROT180, TJXOP_ROT270 }
| Transform operations for tjTransform() More...

## Functions

DLLEXPORT tjhandle DLLCALL | tjInitCompress (void)
| Create a TurboJPEG compressor instance. More...
DLLEXPORT int DLLCALL | tjCompress2 (tjhandle handle, const unsigned char *srcBuf, int width, int pitch, int height, int pixelFormat, unsigned char **jpegBuf, unsigned long *jpegSize, int jpegSubsamp, int jpegQual, int flags)
| Compress an RGB, grayscale, or CMYK image into a JPEG image. More...
DLLEXPORT int DLLCALL | tjCompressFromYUV (tjhandle handle, const unsigned char *srcBuf, int width, int pad, int height, int subsamp, unsigned char **jpegBuf, unsigned long *jpegSize, int jpegQual, int flags)
| Compress a YUV planar image into a JPEG image. More...
DLLEXPORT int DLLCALL | tjCompressFromYUVPlanes (tjhandle handle, const unsigned char **srcPlanes, int width, const int *strides, int height, int subsamp, unsigned char **jpegBuf, unsigned long *jpegSize, int jpegQual, int flags)
| Compress a set of Y, U (Cb), and V (Cr) image planes into a JPEG image. More...
DLLEXPORT unsigned long DLLCALL | tjBufSize (int width, int height, int jpegSubsamp)
| The maximum size of the buffer (in bytes) required to hold a JPEG image with the given parameters. More...
DLLEXPORT unsigned long DLLCALL | tjBufSizeYUV2 (int width, int pad, int height, int subsamp)
| The size of the buffer (in bytes) required to hold a YUV planar image with the given parameters. More...
DLLEXPORT unsigned long DLLCALL | tjPlaneSizeYUV (int componentID, int width, int stride, int height, int subsamp)
| The size of the buffer (in bytes) required to hold a YUV image plane with the given parameters. More...
DLLEXPORT int | tjPlaneWidth (int componentID, int width, int subsamp)
| The plane width of a YUV image plane with the given parameters. More...
DLLEXPORT int | tjPlaneHeight (int componentID, int height, int subsamp)
| The plane height of a YUV image plane with the given parameters. More...
DLLEXPORT int DLLCALL | tjEncodeYUV3 (tjhandle handle, const unsigned char *srcBuf, int width, int pitch, int height, int pixelFormat, unsigned char *dstBuf, int pad, int subsamp, int flags)
| Encode an RGB or grayscale image into a YUV planar image. More...
DLLEXPORT int DLLCALL | tjEncodeYUVPlanes (tjhandle handle, const unsigned char *srcBuf, int width, int pitch, int height, int pixelFormat, unsigned char **dstPlanes, int *strides, int subsamp, int flags)
| Encode an RGB or grayscale image into separate Y, U (Cb), and V (Cr) image planes. More...
DLLEXPORT tjhandle DLLCALL | tjInitDecompress (void)
| Create a TurboJPEG decompressor instance. More...
DLLEXPORT int DLLCALL | tjDecompressHeader3 (tjhandle handle, const unsigned char *jpegBuf, unsigned long jpegSize, int *width, int *height, int *jpegSubsamp, int *jpegColorspace)
| Retrieve information about a JPEG image without decompressing it. More...
DLLEXPORT tjscalingfactor *DLLCALL | tjGetScalingFactors (int *numscalingfactors)
| Returns a list of fractional scaling factors that the JPEG decompressor in this implementation of TurboJPEG supports. More...
DLLEXPORT int DLLCALL | tjDecompress2 (tjhandle handle, const unsigned char *jpegBuf, unsigned long jpegSize, unsigned char *dstBuf, int width, int pitch, int height, int pixelFormat, int flags)
| Decompress a JPEG image to an RGB, grayscale, or CMYK image. More...
DLLEXPORT int DLLCALL | tjDecompressToYUV2 (tjhandle handle, const unsigned char *jpegBuf, unsigned long jpegSize, unsigned char *dstBuf, int width, int pad, int height, int flags)
| Decompress a JPEG image to a YUV planar image. More...
DLLEXPORT int DLLCALL | tjDecompressToYUVPlanes (tjhandle handle, const unsigned char *jpegBuf, unsigned long jpegSize, unsigned char **dstPlanes, int width, int *strides, int height, int flags)
| Decompress a JPEG image into separate Y, U (Cb), and V (Cr) image planes. More...
DLLEXPORT int DLLCALL | tjDecodeYUV (tjhandle handle, const unsigned char *srcBuf, int pad, int subsamp, unsigned char *dstBuf, int width, int pitch, int height, int pixelFormat, int flags)
| Decode a YUV planar image into an RGB or grayscale image. More...
DLLEXPORT int DLLCALL | tjDecodeYUVPlanes (tjhandle handle, const unsigned char **srcPlanes, const int *strides, int subsamp, unsigned char *dstBuf, int width, int pitch, int height, int pixelFormat, int flags)
| Decode a set of Y, U (Cb), and V (Cr) image planes into an RGB or grayscale image. More...
DLLEXPORT tjhandle DLLCALL | tjInitTransform (void)
| Create a new TurboJPEG transformer instance. More...
DLLEXPORT int DLLCALL | tjTransform (tjhandle handle, const unsigned char *jpegBuf, unsigned long jpegSize, int n, unsigned char **dstBufs, unsigned long *dstSizes, tjtransform *transforms, int flags)
| Losslessly transform a JPEG image into another JPEG image. More...
DLLEXPORT int DLLCALL | tjDestroy (tjhandle handle)
| Destroy a TurboJPEG compressor, decompressor, or transformer instance. More...
DLLEXPORT unsigned char *DLLCALL | tjAlloc (int bytes)
| Allocate an image buffer for use with TurboJPEG. More...
DLLEXPORT void DLLCALL | tjFree (unsigned char *buffer)
| Free an image buffer previously allocated by TurboJPEG. More...
DLLEXPORT char *DLLCALL | tjGetErrorStr (void)
| Returns a descriptive error message explaining why the last command failed. More...

## Variables

static const int | tjMCUWidth [TJ_NUMSAMP]
| MCU block width (in pixels) for a given level of chrominance subsampling. More...
static const int | tjMCUHeight [TJ_NUMSAMP]
| MCU block height (in pixels) for a given level of chrominance subsampling. More...
static const int | tjRedOffset [TJ_NUMPF]
| Red offset (in bytes) for a given pixel format. More...
static const int | tjGreenOffset [TJ_NUMPF]
| Green offset (in bytes) for a given pixel format. More...
static const int | tjBlueOffset [TJ_NUMPF]
| Blue offset (in bytes) for a given pixel format. More...
static const int | tjPixelSize [TJ_NUMPF]
| Pixel size (in bytes) for a given pixel format. More...

## Detailed Description

TurboJPEG API.

This API provides an interface for generating, decoding, and transforming planar YUV and JPEG images in memory.

## YUV Image Format Notes

Technically, the JPEG format uses the YCbCr colorspace (which is technically not a colorspace but a color transform), but per the convention of the digital video community, the TurboJPEG API uses "YUV" to refer to an image format consisting of Y, Cb, and Cr image planes.

Each plane is simply a 2D array of bytes, each byte representing the value of one of the components (Y, Cb, or Cr) at a particular location in the image. The width and height of each plane are determined by the image width, height, and level of chrominance subsampling. The luminance plane width is the image width padded to the nearest multiple of the horizontal subsampling factor (2 in the case of 4:2:0 and 4:2:2, 4 in the case of 4:1:1, 1 in the case of 4:4:4 or grayscale.) Similarly, the luminance plane height is the image height padded to the nearest multiple of the vertical subsampling factor (2 in the case of 4:2:0 or 4:4:0, 1 in the case of 4:4:4 or grayscale.) This is irrespective of any additional padding that may be specified as an argument to the various YUV functions. The chrominance plane width is equal to the luminance plane width divided by the horizontal subsampling factor, and the chrominance plane height is equal to the luminance plane height divided by the vertical subsampling factor.

For example, if the source image is 35 x 35 pixels and 4:2:2 subsampling is used, then the luminance plane would be 36 x 35 bytes, and each of the chrominance planes would be 18 x 35 bytes. If you specify a line padding of 4 bytes on top of this, then the luminance plane would be 36 x 35 bytes, and each of the chrominance planes would be 20 x 35 bytes.

## Macro Definition Documentation

#define TJ_NUMCS

The number of JPEG colorspaces.

#define TJ_NUMPF

The number of pixel formats.

#define TJ_NUMSAMP

The number of chrominance subsampling options.

#define TJ_NUMXOP

The number of transform operations.

#define TJFLAG_ACCURATEDCT

Use the most accurate DCT/IDCT algorithm available in the underlying codec.

The default if this flag is not specified is implementation-specific. For example, the implementation of TurboJPEG for libjpeg[-turbo] uses the fast algorithm by default when compressing, because this has been shown to have only a very slight effect on accuracy, but it uses the accurate algorithm when decompressing, because this has been shown to have a larger effect.

#define TJFLAG_BOTTOMUP

The uncompressed source/destination image is stored in bottom-up (Windows, OpenGL) order, not top-down (X11) order.

#define TJFLAG_FASTDCT

Use the fastest DCT/IDCT algorithm available in the underlying codec.

The default if this flag is not specified is implementation-specific. For example, the implementation of TurboJPEG for libjpeg[-turbo] uses the fast algorithm by default when compressing, because this has been shown to have only a very slight effect on accuracy, but it uses the accurate algorithm when decompressing, because this has been shown to have a larger effect.

#define TJFLAG_FASTUPSAMPLE

When decompressing an image that was compressed using chrominance subsampling, use the fastest chrominance upsampling algorithm available in the underlying codec.

The default is to use smooth upsampling, which creates a smooth transition between neighboring chrominance components in order to reduce upsampling artifacts in the decompressed image.

#define TJFLAG_NOREALLOC

Disable buffer (re)allocation.

If passed to one of the JPEG compression or transform functions, this flag will cause those functions to generate an error if the JPEG image buffer is invalid or too small rather than attempting to allocate or reallocate that buffer. This reproduces the behavior of earlier versions of TurboJPEG.

#define TJPAD | ( |  | width | ) |

Pad the given width to the nearest 32-bit boundary.

#define TJSCALED | ( |  | dimension,
|  |  | scalingFactor
| ) |  |

Compute the scaled value of `dimension` using the given scaling factor.

This macro performs the integer equivalent of `ceil(dimension * scalingFactor)`.

#define TJXOPT_CROP

This option will enable lossless cropping.

See tjTransform() for more information.

#define TJXOPT_GRAY

This option will discard the color data in the input image and produce a grayscale output image.

#define TJXOPT_NOOUTPUT

This option will prevent tjTransform() from outputting a JPEG image for this particular transform (this can be used in conjunction with a custom filter to capture the transformed DCT coefficients without transcoding them.)

#define TJXOPT_PERFECT

This option will cause tjTransform() to return an error if the transform is not perfect.

Lossless transforms operate on MCU blocks, whose size depends on the level of chrominance subsampling used (see tjMCUWidth and tjMCUHeight.) If the image's width or height is not evenly divisible by the MCU block size, then there will be partial MCU blocks on the right and/or bottom edges. It is not possible to move these partial MCU blocks to the top or left of the image, so any transform that would require that is "imperfect." If this option is not specified, then any partial MCU blocks that cannot be transformed will be left in place, which will create odd-looking strips on the right or bottom edge of the image.

#define TJXOPT_TRIM

This option will cause tjTransform() to discard any partial MCU blocks that cannot be transformed.

## Typedef Documentation

typedef void* tjhandle

TurboJPEG instance handle.

typedef struct tjtransform tjtransform

Lossless transform.

## Enumeration Type Documentation

enum TJCS

JPEG colorspaces.

Enumerator
TJCS_RGB | RGB colorspace. When compressing the JPEG image, the R, G, and B components in the source image are reordered into image planes, but no colorspace conversion or subsampling is performed. RGB JPEG images can be decompressed to any of the extended RGB pixel formats or grayscale, but they cannot be decompressed to YUV images.
TJCS_YCbCr | YCbCr colorspace. YCbCr is not an absolute colorspace but rather a mathematical transformation of RGB designed solely for storage and transmission. YCbCr images must be converted to RGB before they can actually be displayed. In the YCbCr colorspace, the Y (luminance) component represents the black & white portion of the original image, and the Cb and Cr (chrominance) components represent the color portion of the original image. Originally, the analog equivalent of this transformation allowed the same signal to drive both black & white and color televisions, but JPEG images use YCbCr primarily because it allows the color data to be optionally subsampled for the purposes of reducing bandwidth or disk space. YCbCr is the most common JPEG colorspace, and YCbCr JPEG images can be compressed from and decompressed to any of the extended RGB pixel formats or grayscale, or they can be decompressed to YUV planar images.
TJCS_GRAY | Grayscale colorspace. The JPEG image retains only the luminance data (Y component), and any color data from the source image is discarded. Grayscale JPEG images can be compressed from and decompressed to any of the extended RGB pixel formats or grayscale, or they can be decompressed to YUV planar images.
TJCS_CMYK | CMYK colorspace. When compressing the JPEG image, the C, M, Y, and K components in the source image are reordered into image planes, but no colorspace conversion or subsampling is performed. CMYK JPEG images can only be decompressed to CMYK pixels.
TJCS_YCCK | YCCK colorspace. YCCK (AKA "YCbCrK") is not an absolute colorspace but rather a mathematical transformation of CMYK designed solely for storage and transmission. It is to CMYK as YCbCr is to RGB. CMYK pixels can be reversibly transformed into YCCK, and as with YCbCr, the chrominance components in the YCCK pixels can be subsampled without incurring major perceptual loss. YCCK JPEG images can only be compressed from and decompressed to CMYK pixels.

enum TJPF

Pixel formats.

Enumerator
TJPF_RGB | RGB pixel format. The red, green, and blue components in the image are stored in 3-byte pixels in the order R, G, B from lowest to highest byte address within each pixel.
TJPF_BGR | BGR pixel format. The red, green, and blue components in the image are stored in 3-byte pixels in the order B, G, R from lowest to highest byte address within each pixel.
TJPF_RGBX | RGBX pixel format. The red, green, and blue components in the image are stored in 4-byte pixels in the order R, G, B from lowest to highest byte address within each pixel. The X component is ignored when compressing and undefined when decompressing.
TJPF_BGRX | BGRX pixel format. The red, green, and blue components in the image are stored in 4-byte pixels in the order B, G, R from lowest to highest byte address within each pixel. The X component is ignored when compressing and undefined when decompressing.
TJPF_XBGR | XBGR pixel format. The red, green, and blue components in the image are stored in 4-byte pixels in the order R, G, B from highest to lowest byte address within each pixel. The X component is ignored when compressing and undefined when decompressing.
TJPF_XRGB | XRGB pixel format. The red, green, and blue components in the image are stored in 4-byte pixels in the order B, G, R from highest to lowest byte address within each pixel. The X component is ignored when compressing and undefined when decompressing.
TJPF_GRAY | Grayscale pixel format. Each 1-byte pixel represents a luminance (brightness) level from 0 to 255.
TJPF_RGBA | RGBA pixel format. This is the same as TJPF_RGBX, except that when decompressing, the X component is guaranteed to be 0xFF, which can be interpreted as an opaque alpha channel.
TJPF_BGRA | BGRA pixel format. This is the same as TJPF_BGRX, except that when decompressing, the X component is guaranteed to be 0xFF, which can be interpreted as an opaque alpha channel.
TJPF_ABGR | ABGR pixel format. This is the same as TJPF_XBGR, except that when decompressing, the X component is guaranteed to be 0xFF, which can be interpreted as an opaque alpha channel.
TJPF_ARGB | ARGB pixel format. This is the same as TJPF_XRGB, except that when decompressing, the X component is guaranteed to be 0xFF, which can be interpreted as an opaque alpha channel.
TJPF_CMYK | CMYK pixel format. Unlike RGB, which is an additive color model used primarily for display, CMYK (Cyan/Magenta/Yellow/Key) is a subtractive color model used primarily for printing. In the CMYK color model, the value of each color component typically corresponds to an amount of cyan, magenta, yellow, or black ink that is applied to a white background. In order to convert between CMYK and RGB, it is necessary to use a color management system (CMS.) A CMS will attempt to map colors within the printer's gamut to perceptually similar colors in the display's gamut and vice versa, but the mapping is typically not 1:1 or reversible, nor can it be defined with a simple formula. Thus, such a conversion is out of scope for a codec library. However, the TurboJPEG API allows for compressing CMYK pixels into a YCCK JPEG image (see TJCS_YCCK) and decompressing YCCK JPEG images into CMYK pixels.

enum TJSAMP

Chrominance subsampling options.

When pixels are converted from RGB to YCbCr (see TJCS_YCbCr) or from CMYK to YCCK (see TJCS_YCCK) as part of the JPEG compression process, some of the Cb and Cr (chrominance) components can be discarded or averaged together to produce a smaller image with little perceptible loss of image clarity (the human eye is more sensitive to small changes in brightness than to small changes in color.) This is called "chrominance subsampling".

Enumerator
TJSAMP_444 | 4:4:4 chrominance subsampling (no chrominance subsampling). The JPEG or YUV image will contain one chrominance component for every pixel in the source image.
TJSAMP_422 | 4:2:2 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 2x1 block of pixels in the source image.
TJSAMP_420 | 4:2:0 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 2x2 block of pixels in the source image.
TJSAMP_GRAY | Grayscale. The JPEG or YUV image will contain no chrominance components.
TJSAMP_440 | 4:4:0 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 1x2 block of pixels in the source image.

Note
  4:4:0 subsampling is not fully accelerated in libjpeg-turbo.

TJSAMP_411 | 4:1:1 chrominance subsampling. The JPEG or YUV image will contain one chrominance component for every 4x1 block of pixels in the source image. JPEG images compressed with 4:1:1 subsampling will be almost exactly the same size as those compressed with 4:2:0 subsampling, and in the aggregate, both subsampling methods produce approximately the same perceptual quality. However, 4:1:1 is better able to reproduce sharp horizontal features.

Note
  4:1:1 subsampling is not fully accelerated in libjpeg-turbo.

enum TJXOP

Transform operations for tjTransform()

Enumerator
TJXOP_NONE | Do not transform the position of the image pixels.
TJXOP_HFLIP | Flip (mirror) image horizontally. This transform is imperfect if there are any partial MCU blocks on the right edge (see TJXOPT_PERFECT.)
TJXOP_VFLIP | Flip (mirror) image vertically. This transform is imperfect if there are any partial MCU blocks on the bottom edge (see TJXOPT_PERFECT.)
TJXOP_TRANSPOSE | Transpose image (flip/mirror along upper left to lower right axis.) This transform is always perfect.
TJXOP_TRANSVERSE | Transverse transpose image (flip/mirror along upper right to lower left axis.) This transform is imperfect if there are any partial MCU blocks in the image (see TJXOPT_PERFECT.)
TJXOP_ROT90 | Rotate image clockwise by 90 degrees. This transform is imperfect if there are any partial MCU blocks on the bottom edge (see TJXOPT_PERFECT.)
TJXOP_ROT180 | Rotate image 180 degrees. This transform is imperfect if there are any partial MCU blocks in the image (see TJXOPT_PERFECT.)
TJXOP_ROT270 | Rotate image counter-clockwise by 90 degrees. This transform is imperfect if there are any partial MCU blocks on the right edge (see TJXOPT_PERFECT.)

## Function Documentation

DLLEXPORT unsigned char* DLLCALL tjAlloc | ( | int | bytes | ) |

Allocate an image buffer for use with TurboJPEG.

You should always use this function to allocate the JPEG destination buffer(s) for the compression and transform functions unless you are disabling automatic buffer (re)allocation (by setting TJFLAG_NOREALLOC.)

Parameters

  bytes | the number of bytes to allocate

Returns
  a pointer to a newly-allocated buffer with the specified number of bytes.

See Also
  tjFree()

DLLEXPORT unsigned long DLLCALL tjBufSize | ( | int | width,
|  | int | height,
|  | int | jpegSubsamp
| ) |  |

The maximum size of the buffer (in bytes) required to hold a JPEG image with the given parameters.

The number of bytes returned by this function is larger than the size of the uncompressed source image. The reason for this is that the JPEG format uses 16-bit coefficients, and it is thus possible for a very high-quality JPEG image with very high-frequency content to expand rather than compress when converted to the JPEG format. Such images represent a very rare corner case, but since there is no way to predict the size of a JPEG image prior to compression, the corner case has to be handled.

Parameters

  width | width (in pixels) of the image
  height | height (in pixels) of the image
  jpegSubsamp | the level of chrominance subsampling to be used when generating the JPEG image (see Chrominance subsampling options.)

Returns
  the maximum size of the buffer (in bytes) required to hold the image, or -1 if the arguments are out of bounds.

DLLEXPORT unsigned long DLLCALL tjBufSizeYUV2 | ( | int | width,
|  | int | pad,
|  | int | height,
|  | int | subsamp
| ) |  |

The size of the buffer (in bytes) required to hold a YUV planar image with the given parameters.

Parameters

  width | width (in pixels) of the image
  pad | the width of each line in each plane of the image is padded to the nearest multiple of this number of bytes (must be a power of 2.)
  height | height (in pixels) of the image
  subsamp | level of chrominance subsampling in the image (see Chrominance subsampling options.)

Returns
  the size of the buffer (in bytes) required to hold the image, or -1 if the arguments are out of bounds.

DLLEXPORT int DLLCALL tjCompress2 | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | unsigned char ** | jpegBuf,
|  | unsigned long * | jpegSize,
|  | int | jpegSubsamp,
|  | int | jpegQual,
|  | int | flags
| ) |  |

Compress an RGB, grayscale, or CMYK image into a JPEG image.

Parameters

  handle | a handle to a TurboJPEG compressor or transformer instance
  srcBuf | pointer to an image buffer containing RGB, grayscale, or CMYK pixels to be compressed
  width | width (in pixels) of the source image
  pitch | bytes per line in the source image. Normally, this should be `width * tjPixelSize[pixelFormat]` if the image is unpadded, or `TJPAD(width * tjPixelSize[pixelFormat])` if each line of the image is padded to the nearest 32-bit boundary, as is the case for Windows bitmaps. You can also be clever and use this parameter to skip lines, etc. Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.
  height | height (in pixels) of the source image
  pixelFormat | pixel format of the source image (see Pixel formats.)
  jpegBuf | address of a pointer to an image buffer that will receive the JPEG image. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to:
  1. pre-allocate the JPEG buffer with an arbitrary size using tjAlloc() and let TurboJPEG grow the buffer as needed,
  2. set `*jpegBuf` to NULL to tell TurboJPEG to allocate the buffer for you, or
  3. pre-allocate the buffer to a "worst case" size determined by calling tjBufSize(). This should ensure that the buffer never has to be re-allocated (setting TJFLAG_NOREALLOC guarantees that it won't be.)
  If you choose option 1, `*jpegSize` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJFLAG_NOREALLOC, you should always check `*jpegBuf` upon return from this function, as it may have changed.
  jpegSize | pointer to an unsigned long variable that holds the size of the JPEG image buffer. If `*jpegBuf` points to a pre-allocated buffer, then `*jpegSize` should be set to the size of the buffer. Upon return, `*jpegSize` will contain the size of the JPEG image (in bytes.) If `*jpegBuf` points to a JPEG image buffer that is being reused from a previous call to one of the JPEG compression functions, then `*jpegSize` is ignored.
  jpegSubsamp | the level of chrominance subsampling to be used when generating the JPEG image (see Chrominance subsampling options.)
  jpegQual | the image quality of the generated JPEG image (1 = worst, 100 = best)
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjCompressFromYUV | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | width,
|  | int | pad,
|  | int | height,
|  | int | subsamp,
|  | unsigned char ** | jpegBuf,
|  | unsigned long * | jpegSize,
|  | int | jpegQual,
|  | int | flags
| ) |  |

Compress a YUV planar image into a JPEG image.

Parameters

  handle | a handle to a TurboJPEG compressor or transformer instance
  srcBuf | pointer to an image buffer containing a YUV planar image to be compressed. The size of this buffer should match the value returned by tjBufSizeYUV2() for the given image width, height, padding, and level of chrominance subsampling. The Y, U (Cb), and V (Cr) image planes should be stored sequentially in the source buffer (refer to YUV Image Format Notes.)
  width | width (in pixels) of the source image. If the width is not an even multiple of the MCU block width (see tjMCUWidth), then an intermediate buffer copy will be performed within TurboJPEG.
  pad | the line padding used in the source image. For instance, if each line in each plane of the YUV image is padded to the nearest multiple of 4 bytes, then `pad` should be set to 4.
  height | height (in pixels) of the source image. If the height is not an even multiple of the MCU block height (see tjMCUHeight), then an intermediate buffer copy will be performed within TurboJPEG.
  subsamp | the level of chrominance subsampling used in the source image (see Chrominance subsampling options.)
  jpegBuf | address of a pointer to an image buffer that will receive the JPEG image. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to:
  1. pre-allocate the JPEG buffer with an arbitrary size using tjAlloc() and let TurboJPEG grow the buffer as needed,
  2. set `*jpegBuf` to NULL to tell TurboJPEG to allocate the buffer for you, or
  3. pre-allocate the buffer to a "worst case" size determined by calling tjBufSize(). This should ensure that the buffer never has to be re-allocated (setting TJFLAG_NOREALLOC guarantees that it won't be.)
  If you choose option 1, `*jpegSize` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJFLAG_NOREALLOC, you should always check `*jpegBuf` upon return from this function, as it may have changed.
  jpegSize | pointer to an unsigned long variable that holds the size of the JPEG image buffer. If `*jpegBuf` points to a pre-allocated buffer, then `*jpegSize` should be set to the size of the buffer. Upon return, `*jpegSize` will contain the size of the JPEG image (in bytes.) If `*jpegBuf` points to a JPEG image buffer that is being reused from a previous call to one of the JPEG compression functions, then `*jpegSize` is ignored.
  jpegQual | the image quality of the generated JPEG image (1 = worst, 100 = best)
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjCompressFromYUVPlanes | ( | tjhandle | handle,
|  | const unsigned char ** | srcPlanes,
|  | int | width,
|  | const int * | strides,
|  | int | height,
|  | int | subsamp,
|  | unsigned char ** | jpegBuf,
|  | unsigned long * | jpegSize,
|  | int | jpegQual,
|  | int | flags
| ) |  |

Compress a set of Y, U (Cb), and V (Cr) image planes into a JPEG image.

Parameters

  handle | a handle to a TurboJPEG compressor or transformer instance
  srcPlanes | an array of pointers to Y, U (Cb), and V (Cr) image planes (or just a Y plane, if compressing a grayscale image) that contain a YUV image to be compressed. These planes can be contiguous or non-contiguous in memory. The size of each plane should match the value returned by tjPlaneSizeYUV() for the given image width, height, strides, and level of chrominance subsampling. Refer to YUV Image Format Notes for more details.
  width | width (in pixels) of the source image. If the width is not an even multiple of the MCU block width (see tjMCUWidth), then an intermediate buffer copy will be performed within TurboJPEG.
  strides | an array of integers, each specifying the number of bytes per line in the corresponding plane of the YUV source image. Setting the stride for any plane to 0 is the same as setting it to the plane width (see YUV Image Format Notes.) If `strides` is NULL, then the strides for all planes will be set to their respective plane widths. You can adjust the strides in order to specify an arbitrary amount of line padding in each plane or to create a JPEG image from a subregion of a larger YUV planar image.
  height | height (in pixels) of the source image. If the height is not an even multiple of the MCU block height (see tjMCUHeight), then an intermediate buffer copy will be performed within TurboJPEG.
  subsamp | the level of chrominance subsampling used in the source image (see Chrominance subsampling options.)
  jpegBuf | address of a pointer to an image buffer that will receive the JPEG image. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to:
  1. pre-allocate the JPEG buffer with an arbitrary size using tjAlloc() and let TurboJPEG grow the buffer as needed,
  2. set `*jpegBuf` to NULL to tell TurboJPEG to allocate the buffer for you, or
  3. pre-allocate the buffer to a "worst case" size determined by calling tjBufSize(). This should ensure that the buffer never has to be re-allocated (setting TJFLAG_NOREALLOC guarantees that it won't be.)
  If you choose option 1, `*jpegSize` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJFLAG_NOREALLOC, you should always check `*jpegBuf` upon return from this function, as it may have changed.
  jpegSize | pointer to an unsigned long variable that holds the size of the JPEG image buffer. If `*jpegBuf` points to a pre-allocated buffer, then `*jpegSize` should be set to the size of the buffer. Upon return, `*jpegSize` will contain the size of the JPEG image (in bytes.) If `*jpegBuf` points to a JPEG image buffer that is being reused from a previous call to one of the JPEG compression functions, then `*jpegSize` is ignored.
  jpegQual | the image quality of the generated JPEG image (1 = worst, 100 = best)
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjDecodeYUV | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | pad,
|  | int | subsamp,
|  | unsigned char * | dstBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | int | flags
| ) |  |

Decode a YUV planar image into an RGB or grayscale image.

This function uses the accelerated color conversion routines in the underlying codec but does not execute any of the other steps in the JPEG decompression process.

Parameters

  handle | a handle to a TurboJPEG decompressor or transformer instance
  srcBuf | pointer to an image buffer containing a YUV planar image to be decoded. The size of this buffer should match the value returned by tjBufSizeYUV2() for the given image width, height, padding, and level of chrominance subsampling. The Y, U (Cb), and V (Cr) image planes should be stored sequentially in the source buffer (refer to YUV Image Format Notes.)
  pad | Use this parameter to specify that the width of each line in each plane of the YUV source image is padded to the nearest multiple of this number of bytes (must be a power of 2.)
  subsamp | the level of chrominance subsampling used in the YUV source image (see Chrominance subsampling options.)
  dstBuf | pointer to an image buffer that will receive the decoded image. This buffer should normally be `pitch * height` bytes in size, but the `dstBuf` pointer can also be used to decode into a specific region of a larger buffer.
  width | width (in pixels) of the source and destination images
  pitch | bytes per line in the destination image. Normally, this should be `width * tjPixelSize[pixelFormat]` if the destination image is unpadded, or `TJPAD(width * tjPixelSize[pixelFormat])` if each line of the destination image should be padded to the nearest 32-bit boundary, as is the case for Windows bitmaps. You can also be clever and use the pitch parameter to skip lines, etc. Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.
  height | height (in pixels) of the source and destination images
  pixelFormat | pixel format of the destination image (see Pixel formats.)
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjDecodeYUVPlanes | ( | tjhandle | handle,
|  | const unsigned char ** | srcPlanes,
|  | const int * | strides,
|  | int | subsamp,
|  | unsigned char * | dstBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | int | flags
| ) |  |

Decode a set of Y, U (Cb), and V (Cr) image planes into an RGB or grayscale image.

This function uses the accelerated color conversion routines in the underlying codec but does not execute any of the other steps in the JPEG decompression process.

Parameters

  handle | a handle to a TurboJPEG decompressor or transformer instance
  srcPlanes | an array of pointers to Y, U (Cb), and V (Cr) image planes (or just a Y plane, if decoding a grayscale image) that contain a YUV image to be decoded. These planes can be contiguous or non-contiguous in memory. The size of each plane should match the value returned by tjPlaneSizeYUV() for the given image width, height, strides, and level of chrominance subsampling. Refer to YUV Image Format Notes for more details.
  strides | an array of integers, each specifying the number of bytes per line in the corresponding plane of the YUV source image. Setting the stride for any plane to 0 is the same as setting it to the plane width (see YUV Image Format Notes.) If `strides` is NULL, then the strides for all planes will be set to their respective plane widths. You can adjust the strides in order to specify an arbitrary amount of line padding in each plane or to decode a subregion of a larger YUV planar image.
  subsamp | the level of chrominance subsampling used in the YUV source image (see Chrominance subsampling options.)
  dstBuf | pointer to an image buffer that will receive the decoded image. This buffer should normally be `pitch * height` bytes in size, but the `dstBuf` pointer can also be used to decode into a specific region of a larger buffer.
  width | width (in pixels) of the source and destination images
  pitch | bytes per line in the destination image. Normally, this should be `width * tjPixelSize[pixelFormat]` if the destination image is unpadded, or `TJPAD(width * tjPixelSize[pixelFormat])` if each line of the destination image should be padded to the nearest 32-bit boundary, as is the case for Windows bitmaps. You can also be clever and use the pitch parameter to skip lines, etc. Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.
  height | height (in pixels) of the source and destination images
  pixelFormat | pixel format of the destination image (see Pixel formats.)
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjDecompress2 | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | unsigned long | jpegSize,
|  | unsigned char * | dstBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | int | flags
| ) |  |

Decompress a JPEG image to an RGB, grayscale, or CMYK image.

Parameters

  handle | a handle to a TurboJPEG decompressor or transformer instance
  jpegBuf | pointer to a buffer containing the JPEG image to decompress
  jpegSize | size of the JPEG image (in bytes)
  dstBuf | pointer to an image buffer that will receive the decompressed image. This buffer should normally be `pitch * scaledHeight` bytes in size, where `scaledHeight` can be determined by calling TJSCALED() with the JPEG image height and one of the scaling factors returned by tjGetScalingFactors(). The `dstBuf` pointer may also be used to decompress into a specific region of a larger buffer.
  width | desired width (in pixels) of the destination image. If this is different than the width of the JPEG image being decompressed, then TurboJPEG will use scaling in the JPEG decompressor to generate the largest possible image that will fit within the desired width. If `width` is set to 0, then only the height will be considered when determining the scaled image size.
  pitch | bytes per line in the destination image. Normally, this is `scaledWidth * tjPixelSize[pixelFormat]` if the decompressed image is unpadded, else `TJPAD(scaledWidth * tjPixelSize[pixelFormat])` if each line of the decompressed image is padded to the nearest 32-bit boundary, as is the case for Windows bitmaps. (NOTE: `scaledWidth` can be determined by calling TJSCALED() with the JPEG image width and one of the scaling factors returned by tjGetScalingFactors().) You can also be clever and use the pitch parameter to skip lines, etc. Setting this parameter to 0 is the equivalent of setting it to `scaledWidth * tjPixelSize[pixelFormat]`.
  height | desired height (in pixels) of the destination image. If this is different than the height of the JPEG image being decompressed, then TurboJPEG will use scaling in the JPEG decompressor to generate the largest possible image that will fit within the desired height. If `height` is set to 0, then only the width will be considered when determining the scaled image size.
  pixelFormat | pixel format of the destination image (see Pixel formats.)
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjDecompressHeader3 | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | unsigned long | jpegSize,
|  | int * | width,
|  | int * | height,
|  | int * | jpegSubsamp,
|  | int * | jpegColorspace
| ) |  |

Retrieve information about a JPEG image without decompressing it.

Parameters

  handle | a handle to a TurboJPEG decompressor or transformer instance
  jpegBuf | pointer to a buffer containing a JPEG image
  jpegSize | size of the JPEG image (in bytes)
  width | pointer to an integer variable that will receive the width (in pixels) of the JPEG image
  height | pointer to an integer variable that will receive the height (in pixels) of the JPEG image
  jpegSubsamp | pointer to an integer variable that will receive the level of chrominance subsampling used when the JPEG image was compressed (see Chrominance subsampling options.)
  jpegColorspace | pointer to an integer variable that will receive one of the JPEG colorspace constants, indicating the colorspace of the JPEG image (see JPEG colorspaces.)

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjDecompressToYUV2 | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | unsigned long | jpegSize,
|  | unsigned char * | dstBuf,
|  | int | width,
|  | int | pad,
|  | int | height,
|  | int | flags
| ) |  |

Decompress a JPEG image to a YUV planar image.

This function performs JPEG decompression but leaves out the color conversion step, so a planar YUV image is generated instead of an RGB image.

Parameters

  handle | a handle to a TurboJPEG decompressor or transformer instance
  jpegBuf | pointer to a buffer containing the JPEG image to decompress
  jpegSize | size of the JPEG image (in bytes)
  dstBuf | pointer to an image buffer that will receive the YUV image. Use tjBufSizeYUV2() to determine the appropriate size for this buffer based on the image width, height, padding, and level of subsampling. The Y, U (Cb), and V (Cr) image planes will be stored sequentially in the buffer (refer to YUV Image Format Notes.)
  width | desired width (in pixels) of the YUV image. If this is different than the width of the JPEG image being decompressed, then TurboJPEG will use scaling in the JPEG decompressor to generate the largest possible image that will fit within the desired width. If `width` is set to 0, then only the height will be considered when determining the scaled image size. If the scaled width is not an even multiple of the MCU block width (see tjMCUWidth), then an intermediate buffer copy will be performed within TurboJPEG.
  pad | the width of each line in each plane of the YUV image will be padded to the nearest multiple of this number of bytes (must be a power of 2.) To generate images suitable for X Video, `pad` should be set to 4.
  height | desired height (in pixels) of the YUV image. If this is different than the height of the JPEG image being decompressed, then TurboJPEG will use scaling in the JPEG decompressor to generate the largest possible image that will fit within the desired height. If `height` is set to 0, then only the width will be considered when determining the scaled image size. If the scaled height is not an even multiple of the MCU block height (see tjMCUHeight), then an intermediate buffer copy will be performed within TurboJPEG.
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjDecompressToYUVPlanes | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | unsigned long | jpegSize,
|  | unsigned char ** | dstPlanes,
|  | int | width,
|  | int * | strides,
|  | int | height,
|  | int | flags
| ) |  |

Decompress a JPEG image into separate Y, U (Cb), and V (Cr) image planes.

This function performs JPEG decompression but leaves out the color conversion step, so a planar YUV image is generated instead of an RGB image.

Parameters

  handle | a handle to a TurboJPEG decompressor or transformer instance
  jpegBuf | pointer to a buffer containing the JPEG image to decompress
  jpegSize | size of the JPEG image (in bytes)
  dstPlanes | an array of pointers to Y, U (Cb), and V (Cr) image planes (or just a Y plane, if decompressing a grayscale image) that will receive the YUV image. These planes can be contiguous or non-contiguous in memory. Use tjPlaneSizeYUV() to determine the appropriate size for each plane based on the scaled image width, scaled image height, strides, and level of chrominance subsampling. Refer to YUV Image Format Notes for more details.
  width | desired width (in pixels) of the YUV image. If this is different than the width of the JPEG image being decompressed, then TurboJPEG will use scaling in the JPEG decompressor to generate the largest possible image that will fit within the desired width. If `width` is set to 0, then only the height will be considered when determining the scaled image size. If the scaled width is not an even multiple of the MCU block width (see tjMCUWidth), then an intermediate buffer copy will be performed within TurboJPEG.
  strides | an array of integers, each specifying the number of bytes per line in the corresponding plane of the output image. Setting the stride for any plane to 0 is the same as setting it to the scaled plane width (see YUV Image Format Notes.) If `strides` is NULL, then the strides for all planes will be set to their respective scaled plane widths. You can adjust the strides in order to add an arbitrary amount of line padding to each plane or to decompress the JPEG image into a subregion of a larger YUV planar image.
  height | desired height (in pixels) of the YUV image. If this is different than the height of the JPEG image being decompressed, then TurboJPEG will use scaling in the JPEG decompressor to generate the largest possible image that will fit within the desired height. If `height` is set to 0, then only the width will be considered when determining the scaled image size. If the scaled height is not an even multiple of the MCU block height (see tjMCUHeight), then an intermediate buffer copy will be performed within TurboJPEG.
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjDestroy | ( | tjhandle | handle | ) |

Destroy a TurboJPEG compressor, decompressor, or transformer instance.

Parameters

  handle | a handle to a TurboJPEG compressor, decompressor or transformer instance

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjEncodeYUV3 | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | unsigned char * | dstBuf,
|  | int | pad,
|  | int | subsamp,
|  | int | flags
| ) |  |

Encode an RGB or grayscale image into a YUV planar image.

This function uses the accelerated color conversion routines in the underlying codec but does not execute any of the other steps in the JPEG compression process.

Parameters

  handle | a handle to a TurboJPEG compressor or transformer instance
  srcBuf | pointer to an image buffer containing RGB or grayscale pixels to be encoded
  width | width (in pixels) of the source image
  pitch | bytes per line in the source image. Normally, this should be `width * tjPixelSize[pixelFormat]` if the image is unpadded, or `TJPAD(width * tjPixelSize[pixelFormat])` if each line of the image is padded to the nearest 32-bit boundary, as is the case for Windows bitmaps. You can also be clever and use this parameter to skip lines, etc. Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.
  height | height (in pixels) of the source image
  pixelFormat | pixel format of the source image (see Pixel formats.)
  dstBuf | pointer to an image buffer that will receive the YUV image. Use tjBufSizeYUV2() to determine the appropriate size for this buffer based on the image width, height, padding, and level of chrominance subsampling. The Y, U (Cb), and V (Cr) image planes will be stored sequentially in the buffer (refer to YUV Image Format Notes.)
  pad | the width of each line in each plane of the YUV image will be padded to the nearest multiple of this number of bytes (must be a power of 2.) To generate images suitable for X Video, `pad` should be set to 4.
  subsamp | the level of chrominance subsampling to be used when generating the YUV image (see Chrominance subsampling options.) To generate images suitable for X Video, `subsamp` should be set to TJSAMP_420. This produces an image compatible with the I420 (AKA "YUV420P") format.
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT int DLLCALL tjEncodeYUVPlanes | ( | tjhandle | handle,
|  | const unsigned char * | srcBuf,
|  | int | width,
|  | int | pitch,
|  | int | height,
|  | int | pixelFormat,
|  | unsigned char ** | dstPlanes,
|  | int * | strides,
|  | int | subsamp,
|  | int | flags
| ) |  |

Encode an RGB or grayscale image into separate Y, U (Cb), and V (Cr) image planes.

This function uses the accelerated color conversion routines in the underlying codec but does not execute any of the other steps in the JPEG compression process.

Parameters

  handle | a handle to a TurboJPEG compressor or transformer instance
  srcBuf | pointer to an image buffer containing RGB or grayscale pixels to be encoded
  width | width (in pixels) of the source image
  pitch | bytes per line in the source image. Normally, this should be `width * tjPixelSize[pixelFormat]` if the image is unpadded, or `TJPAD(width * tjPixelSize[pixelFormat])` if each line of the image is padded to the nearest 32-bit boundary, as is the case for Windows bitmaps. You can also be clever and use this parameter to skip lines, etc. Setting this parameter to 0 is the equivalent of setting it to `width * tjPixelSize[pixelFormat]`.
  height | height (in pixels) of the source image
  pixelFormat | pixel format of the source image (see Pixel formats.)
  dstPlanes | an array of pointers to Y, U (Cb), and V (Cr) image planes (or just a Y plane, if generating a grayscale image) that will receive the encoded image. These planes can be contiguous or non-contiguous in memory. Use tjPlaneSizeYUV() to determine the appropriate size for each plane based on the image width, height, strides, and level of chrominance subsampling. Refer to YUV Image Format Notes for more details.
  strides | an array of integers, each specifying the number of bytes per line in the corresponding plane of the output image. Setting the stride for any plane to 0 is the same as setting it to the plane width (see YUV Image Format Notes.) If `strides` is NULL, then the strides for all planes will be set to their respective plane widths. You can adjust the strides in order to add an arbitrary amount of line padding to each plane or to encode an RGB or grayscale image into a subregion of a larger YUV planar image.
  subsamp | the level of chrominance subsampling to be used when generating the YUV image (see Chrominance subsampling options.) To generate images suitable for X Video, `subsamp` should be set to TJSAMP_420. This produces an image compatible with the I420 (AKA "YUV420P") format.
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

DLLEXPORT void DLLCALL tjFree | ( | unsigned char * | buffer | ) |

Free an image buffer previously allocated by TurboJPEG.

You should always use this function to free JPEG destination buffer(s) that were automatically (re)allocated by the compression and transform functions or that were manually allocated using tjAlloc().

Parameters

  buffer | address of the buffer to free

See Also
  tjAlloc()

DLLEXPORT char* DLLCALL tjGetErrorStr | ( | void |  | ) |

Returns a descriptive error message explaining why the last command failed.

Returns
  a descriptive error message explaining why the last command failed.

DLLEXPORT tjscalingfactor* DLLCALL tjGetScalingFactors | ( | int * | numscalingfactors | ) |

Returns a list of fractional scaling factors that the JPEG decompressor in this implementation of TurboJPEG supports.

Parameters

  numscalingfactors | pointer to an integer variable that will receive the number of elements in the list

Returns
  a pointer to a list of fractional scaling factors, or NULL if an error is encountered (see tjGetErrorStr().)

DLLEXPORT tjhandle DLLCALL tjInitCompress | ( | void |  | ) |

Create a TurboJPEG compressor instance.

Returns
  a handle to the newly-created instance, or NULL if an error occurred (see tjGetErrorStr().)

DLLEXPORT tjhandle DLLCALL tjInitDecompress | ( | void |  | ) |

Create a TurboJPEG decompressor instance.

Returns
  a handle to the newly-created instance, or NULL if an error occurred (see tjGetErrorStr().)

DLLEXPORT tjhandle DLLCALL tjInitTransform | ( | void |  | ) |

Create a new TurboJPEG transformer instance.

Returns
  a handle to the newly-created instance, or NULL if an error occurred (see tjGetErrorStr().)

DLLEXPORT int tjPlaneHeight | ( | int | componentID,
|  | int | height,
|  | int | subsamp
| ) |  |

The plane height of a YUV image plane with the given parameters.

Refer to YUV Image Format Notes for a description of plane height.

Parameters

  componentID | ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
  height | height (in pixels) of the YUV image
  subsamp | level of chrominance subsampling in the image (see Chrominance subsampling options.)

Returns
  the plane height of a YUV image plane with the given parameters, or -1 if the arguments are out of bounds.

DLLEXPORT unsigned long DLLCALL tjPlaneSizeYUV | ( | int | componentID,
|  | int | width,
|  | int | stride,
|  | int | height,
|  | int | subsamp
| ) |  |

The size of the buffer (in bytes) required to hold a YUV image plane with the given parameters.

Parameters

  componentID | ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
  width | width (in pixels) of the YUV image. NOTE: this is the width of the whole image, not the plane width.
  stride | bytes per line in the image plane. Setting this to 0 is the equivalent of setting it to the plane width.
  height | height (in pixels) of the YUV image. NOTE: this is the height of the whole image, not the plane height.
  subsamp | level of chrominance subsampling in the image (see Chrominance subsampling options.)

Returns
  the size of the buffer (in bytes) required to hold the YUV image plane, or -1 if the arguments are out of bounds.

DLLEXPORT int tjPlaneWidth | ( | int | componentID,
|  | int | width,
|  | int | subsamp
| ) |  |

The plane width of a YUV image plane with the given parameters.

Refer to YUV Image Format Notes for a description of plane width.

Parameters

  componentID | ID number of the image plane (0 = Y, 1 = U/Cb, 2 = V/Cr)
  width | width (in pixels) of the YUV image
  subsamp | level of chrominance subsampling in the image (see Chrominance subsampling options.)

Returns
  the plane width of a YUV image plane with the given parameters, or -1 if the arguments are out of bounds.

DLLEXPORT int DLLCALL tjTransform | ( | tjhandle | handle,
|  | const unsigned char * | jpegBuf,
|  | unsigned long | jpegSize,
|  | int | n,
|  | unsigned char ** | dstBufs,
|  | unsigned long * | dstSizes,
|  | tjtransform * | transforms,
|  | int | flags
| ) |  |

Losslessly transform a JPEG image into another JPEG image.

Lossless transforms work by moving the raw DCT coefficients from one JPEG image structure to another without altering the values of the coefficients. While this is typically faster than decompressing the image, transforming it, and re-compressing it, lossless transforms are not free. Each lossless transform requires reading and performing Huffman decoding on all of the coefficients in the source image, regardless of the size of the destination image. Thus, this function provides a means of generating multiple transformed images from the same source or applying multiple transformations simultaneously, in order to eliminate the need to read the source coefficients multiple times.

Parameters

  handle | a handle to a TurboJPEG transformer instance
  jpegBuf | pointer to a buffer containing the JPEG source image to transform
  jpegSize | size of the JPEG source image (in bytes)
  n | the number of transformed JPEG images to generate
  dstBufs | pointer to an array of n image buffers. `dstBufs[i]` will receive a JPEG image that has been transformed using the parameters in `transforms[i]`. TurboJPEG has the ability to reallocate the JPEG buffer to accommodate the size of the JPEG image. Thus, you can choose to:
  1. pre-allocate the JPEG buffer with an arbitrary size using tjAlloc() and let TurboJPEG grow the buffer as needed,
  2. set `dstBufs[i]` to NULL to tell TurboJPEG to allocate the buffer for you, or
  3. pre-allocate the buffer to a "worst case" size determined by calling tjBufSize() with the transformed or cropped width and height. Under normal circumstances, this should ensure that the buffer never has to be re-allocated (setting TJFLAG_NOREALLOC guarantees that it won't be.) Note, however, that there are some rare cases (such as transforming images with a large amount of embedded EXIF or ICC profile data) in which the output image will be larger than the worst-case size, and TJFLAG_NOREALLOC cannot be used in those cases.
  If you choose option 1, `dstSizes[i]` should be set to the size of your pre-allocated buffer. In any case, unless you have set TJFLAG_NOREALLOC, you should always check `dstBufs[i]` upon return from this function, as it may have changed.
  dstSizes | pointer to an array of n unsigned long variables that will receive the actual sizes (in bytes) of each transformed JPEG image. If `dstBufs[i]` points to a pre-allocated buffer, then `dstSizes[i]` should be set to the size of the buffer. Upon return, `dstSizes[i]` will contain the size of the JPEG image (in bytes.)
  transforms | pointer to an array of n tjtransform structures, each of which specifies the transform parameters and/or cropping region for the corresponding transformed output image.
  flags | the bitwise OR of one or more of the flags

Returns
  0 if successful, or -1 if an error occurred (see tjGetErrorStr().)

## Variable Documentation

const int tjBlueOffset[TJ_NUMPF]

static

Blue offset (in bytes) for a given pixel format.

This specifies the number of bytes that the Blue component is offset from the start of the pixel. For instance, if a pixel of format TJ_BGRX is stored in `char pixel[]`, then the blue component will be `pixel[tjBlueOffset[TJ_BGRX]]`.

const int tjGreenOffset[TJ_NUMPF]

static

Green offset (in bytes) for a given pixel format.

This specifies the number of bytes that the green component is offset from the start of the pixel. For instance, if a pixel of format TJ_BGRX is stored in `char pixel[]`, then the green component will be `pixel[tjGreenOffset[TJ_BGRX]]`.

const int tjMCUHeight[TJ_NUMSAMP]

static

MCU block height (in pixels) for a given level of chrominance subsampling.

MCU block sizes:

- 8x8 for no subsampling or grayscale
- 16x8 for 4:2:2
- 8x16 for 4:4:0
- 16x16 for 4:2:0
- 32x8 for 4:1:1

const int tjMCUWidth[TJ_NUMSAMP]

static

MCU block width (in pixels) for a given level of chrominance subsampling.

MCU block sizes:

- 8x8 for no subsampling or grayscale
- 16x8 for 4:2:2
- 8x16 for 4:4:0
- 16x16 for 4:2:0
- 32x8 for 4:1:1

const int tjPixelSize[TJ_NUMPF]

static

Pixel size (in bytes) for a given pixel format.

const int tjRedOffset[TJ_NUMPF]

static

Red offset (in bytes) for a given pixel format.

This specifies the number of bytes that the red component is offset from the start of the pixel. For instance, if a pixel of format TJ_BGRX is stored in `char pixel[]`, then the red component will be `pixel[tjRedOffset[TJ_BGRX]]`.