


 APRS operates around several primary display screens.  These screens display
 either the APRS MAPs or information accumulated on all packets heard.   Hit
 the SPACE BAR to see the map or the following keys for other displays:

     L - LATEST Beacons     D - DIGI's used     R - READ TRAFFIC
     P - POSITIONS list     H - HEARD log       V - VIEW all packets
     B - BULLETINS          A - ALL BEACONS     alt-T TELEMETRY Page

 Message TRAFFIC can be displayd using the T command and managed as follows:

     S - SEND traffic       K - KILL traffic    E - ERASE outgoing lines    

 Most other APRS functions are accessed in the following SUB MENU's:

     C - CONTROLS           F - FILES           I - INPUT POSITIONS
     M - MAP FUNCTIONS      O - OPERATIONS      W - WEATHER Functions
     F1- HELP MENU !!!      alt-S SETUP menu

 This screen will NOT show again, unless you select NEW on the F1-HELP menu.

