  WELCOME NEW REGISTERED USER!  

  Now that your copy of APRS is validated, your SETUP and CONFIGURATION will
  be saved in a config file.  APRS will always check for a CONFIG file with
  the extension of .APR  unless another 3 character  extension is specified.
  Be sure you have 1) placed yourself on the map,
                   2) centered the map to your area of interest,
                   3) entered a digipeater path using the UNPROTO command
  These will establish where APRS begins each session.  If you want to change
  these, you may do so at anytime and re-save your SETUP and CONFIG file. You
  may also save other  config files under different  3 character extensions.
  These may then be activated from DOS by adding the /xxx extension:
                   FOR EXAMPLE:  C:\APRS> APRS63/GPS.
  Each extension can be a different application,  GPS, WX, MOB, HF, etc.  To
  over-ride the .APR config, or to re-start APRS from scratch, simply specify
  an extension that does not exist such as C:\APRS> APRS63/new.

  Thank you for contributing to the APRS idea.  I hope you find it useful...

